# AMWA IS-09 NMOS System Parameters Specification

[![Lint Status](https://github.com/AMWA-TV/is-09/workflows/Lint/badge.svg)](https://github.com/AMWA-TV/is-09/actions?query=workflow%3ALint)
[![Render Status](https://github.com/AMWA-TV/is-09/workflows/Render/badge.svg)](https://github.com/AMWA-TV/is-09/actions?query=workflow%3ARender)

<!-- INTRO-START -->

### What does it do?

- Allows an NMOS Node (also known as a "Media Node") to obtain global configuration parameters that are common across the system.

### Why does it matter?

- Enables the Node to start, or re-start, in a well defined way that is consistent with the environment it's running in.

### How does it work?

- Defines the System API 'global configuration resource' and the expected behaviour for Nodes using it.

<!-- INTRO-END -->

## Getting started

There is more information about the NMOS Specifications and their GitHub repos at <https://specs.amwa.tv/nmos>.
