# Behaviour: MQTT Transport Type

_(c) AMWA 2017, CC Attribution-NoDerivatives 4.0 International (CC BY-ND 4.0)_

## Transport File Resource

The Sender `/transportfile` resource SHOULD NOT be used for this transport type. This resource SHOULD return a `404` (Not Found) error code if requested.

## Parameter Sets

Sender and Receiver Connection Management endpoints MUST support a core parameter set as follows.

### Receiver Parameter Sets

#### Core Parameters

- `source_host`
- `source_port`
- `broker_topic`
- `broker_protocol`
- `broker_authorization`
- `connection_status_broker_topic`

### Sender Parameter Sets

#### Core Parameters

- `destination_host`
- `destination_port`
- `broker_topic`
- `broker_protocol`
- `broker_authorization`
- `connection_status_broker_topic`

## Use of auto

Parameters which support use of `auto` are identified in the schemas.
